<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="27.92" y2="0" width="0" layer="20"/>
<wire x1="27.92" y1="0" x2="27.92" y2="21.26" width="0" layer="20"/>
<wire x1="27.92" y1="21.26" x2="0" y2="21.26" width="0" layer="20"/>
<wire x1="0" y1="21.26" x2="0" y2="0" width="0" layer="20"/>
<text>TDI</text>
<text>TDO</text>
<text>/RST</text>
<text>TX</text>
<text>RX</text>
<text>GND</text>
<text>TMS/IO</text>
<text>3V3</text>
<text>5V</text>
<text>TCK/CK</text>
<text>TX</text>
<text>RX</text>
<text>GND</text>
<text>TDI</text>
<text>TDO</text>
<text>/RST</text>
<text>TX</text>
<text>RX</text>
<text>TCK/CK</text>
<text>GND</text>
<text>TMS/IO</text>
<text>3V3</text>
<text>5V</text>
<text>NanoDapAdapter
v1</text>
</plain>
<libraries>
<library name="rickk2">
<packages>
<package name="JTAG-MICRO-2X5">
</package>
<package name="1X05">
</package>
<package name="1X03">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="rickk2" package="JTAG-MICRO-2X5" value="JTAG-MICRO-2X5"/>
<element name="JP1" library="rickk2" package="1X05" value="M05PTH"/>
<element name="JP2" library="rickk2" package="1X05" value="M05PTH"/>
<element name="U$1" library="rickk2" package="1X03" value="M03"/>
</elements>
<signals>
<signal name="/RST">
<contactref element="JP2" pad="3"/>
<contactref element="J1" pad="10"/>
</signal>
<signal name="TX">
<contactref element="JP2" pad="2"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="RX">
<contactref element="JP2" pad="1"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="3V3">
<contactref element="JP1" pad="2"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="SWDIO">
<contactref element="JP1" pad="3"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="SWCLK">
<contactref element="JP1" pad="5"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="GND">
<contactref element="JP1" pad="4"/>
<contactref element="J1" pad="3"/>
<contactref element="J1" pad="5"/>
<contactref element="J1" pad="9"/>
<contactref element="U$1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
